[image: image1.png]



Ref: IGV031

Video of the Week – How chainflex bus cables suit all moving applications

In this week’s video, learn about the quality design features for high-end bus cables, and their critical importance for engineers building moving systems in energy chains. 
Low-end “chain-suitable” bus cables usually feature simple extruded outer jackets and open shielding, which in dynamic motion can lead to abrasion damage and interference. They also tend to have a layered design with poor guidance of conductors, resulting in lower signal quality. 
Conversely, high-end bus cables, such as chainflex bus cables, feature pressure extruded outer jackets and optimised shield braiding. They are designed to stand up to dynamic continuous motion with high cycle rates, resulting in reliable and durable EMC safety. Short pitch winding and pressure extruded inner jackets also ensure high signal quality at all times. 
igus chainflex bus cables are designed to work flawlessly over long periods, withstanding millions of cycles and extreme ambient conditions, as well as torsion, and high speeds and accelerations. Tested in e-chains over many millions of cycles at the state-of-the-art igus test laboratory in Cologne, Germany, they provide guaranteed safety against failure, with 36 months’ warranty, reliable service life calculations and options for condition monitoring and predictive maintenance.
See for yourself, visit: www.igus.co.uk/chainflexbuscableVOTW
For more information on igus products and to request free product samples, please visit: www.igus.co.uk/chainflex or call igus directly on: 01604 677240
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	LiveChat with our technical team at igus.co.uk
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	Follow us at twitter.com/igusUK 

	[image: image4.jpg]luf:)




	Watch our videos at igus.co.uk/YouTube
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	Connect to us at igus.co.uk/Facebook 

	
	Read our blog at blog.igus.co.uk 


About igus:

Based in Northampton in the UK and with global headquarters in Cologne, Germany, igus is a leading international manufacturer of energy chain systems and polymer plain bearings. The family-run company is represented in 35 countries and employs 4,150 people around the world. In 2018, igus generated a turnover of 748 million euros with motion plastics, plastic components for moving applications.

With plastic bearing experience since 1964, cable carrier experience since 1971 and continuous-flex cable experience since 1989, igus provides the right solution based on 100,000 products available from stock, with between 1,500 and 2,500 new product introductions each year. igus operates the largest test laboratories and factories in its sector to offer customers quick turnaround times on innovative products and solutions tailored to their needs.

The terms igus, Apiro, chainflex, CFRIP, conprotect, CTD, drylin, dry-tech, dryspin, easy chain, e-chain, e-chain systems, e-ketten, e-kettensysteme, e-skin, flizz, ibow, igear, iglidur, igubal, kineKIT, manus, motion plastics, pikchain, plastics for longer life, readychain, readycable, ReBeL, speedigus, triflex, robolink, and xiros are protected by trademark laws in the Federal Republic of Germany and internationally, where applicable.

All other registered trademarks and trademarks are the property of their respective owners.
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